It was gonna be a carms solve... but my first attempt at 1 arm solving invalidated it for that. could be a sum solve... but any min cycles with existent secondary optimization beats it there. idk, cycles+(cost+area)*2 or something