Shaved 1 area by turning wasted area into track then splitting the work of the piston into 2 arms on the track

Feels like min primary will be <90.
Min area is 16, so hard minimum is 69, but practically can't have low period on that low of an area