i think this is the first time i've had to take a derivative to solve for optimal rate (throughput? i think i might've mixed them up and am genuinely not sure which is which anymore). i am terribly sorry about the amount of instructions but you know what they say: sometimes you gotta make your tertiary worse by 26k to improve your primary by 0.003