I believe the ??? metric is some increasing function of rate, with the secondary and tertiary being cost and instructions. This solution should have min rate, with two water being output each cycle. Initially I tried to make this entirely symmetrical, but using two hexarms for the disposal caused some problems.