Halt arms don't contribute to machine period. This is a period 0 min area solution, so it gets a score of 48 in the second metric. You're not getting min area with the length-2 fixed arm necessary to reach Disposal, so the only thing that matters is the instructions tertiary, which equals the cycle count when you're using a Halt arm. So without the finite rate restriction, this metric would just be AC.