@V is so annoying why is it not @inf smh. It would be so much more convenient if I could just chain the waste instead of making the solution 5P.

I can see potentially saving gold by bonding the lead onto the far side of the product, then debonding and chaining it on the other end without using a piston, but I don't see how that would be possible cheaply enough.