The pipelines have 2 regrabs, one right away, and one after the last debond. The second regrab was a thinko, but I didn't have time to look for a better layout.

The fact that I couldn't get the output directly above the input will haunt me. Making the right pipeline drop off one hex over cost 65G, though it does make the two different disposal pieplines pretty cool. No waste chain is a nice plus too.

I look forward to seeing the madwoman who gets sub-24.